
PCI Power Management
~~~~~~~~~~~~~~~~~~~~

An overview of the concepts and the related functions in the Linux kernel

Patrick Mochel <mochel@transmeta.com>

---------------------------------------------------------------------------

1. Overview
2. How the PCI Subsystem Does Power Management
3. PCI Utility Functions
4. PCI Device Drivers
5. Resources

1. Overview
~~~~~~~~~~~

The PCI Power Management Specification was introduced between the PCI 2.1 and
PCI 2.2 Specifications. It a standard interface for controlling various 
power management operations.

Implementation of the PCI PM Spec is optional, as are several sub-components of
it. If a device supports the PCI PM Spec, the device will have an 8 byte
capability field in its PCI configuration space. This field is used to describe
and control the standard PCI power management features.

The PCI PM spec defines 4 operating states for devices (D0 - D3) and for buses
(B0 - B3). The higher the number, the less power the device consumes. However,
the higher the number, the longer the latency is for the device to return to 
an operational state (D0).

Bus power management is not covered in this version of this document.

Note that all PCI devices support D0 and D3 by default, regardless of whether or
not they implement any of the PCI PM spec.

The possible state transitions that a device can undergo are:

+---------------------------+
| Current State | New State |
+---------------------------+
| D0            | D1, D2, D3|
+---------------------------+
| D1            | D2, D3    |
+---------------------------+
| D2            | D3        |
+---------------------------+
| D1, D2, D3    | D0        |
+---------------------------+

Note that when the system is entering a global suspend state, all devices will
be placed into D3 and when resuming, all devices will be placed into D0.
However, when the system is running, other state transitions are possible.

2. How The PCI Subsystem Handles Power Management
~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~

The PCI suspend/resume functionality is accessed indirectly via the Power
Management subsystem. At boot, the PCI driver registers a power management
callback with that layer. Upon entering a suspend state, the PM layer iterates
through all of its registered callbacks. This currently takes place only during
APM state transitions.

Upon going to sleep, the PCI subsystem walks its device tree twice. Both times,
it does a depth first walk of the device tree. The first walk saves each of the
device's state and checks for devices that will prevent the system from entering
a global power state. The next walk then places the devices in a low power
state.

The first walk allows a graceful recovery in the event of a failure, since none
of the devices have actually been powered down.

In both walks, in particular the second, all children of a bridge are touched
before the actual bridge itself. This allows the bridge to retain power while
its children are being accessed.

Upon resuming from sleep, just the opposite must be true: all bridges must be
powered on and restored before their children are powered on. This is easily
accomplished with a breadth-first walk of the PCI device tree.


3. PCI Utility Functions
~~~~~~~~~~~~~~~~~~~~~~~~

These are helper functions designed to be called by individual device drivers.
Assuming that a device behaves as advertised, these should be applicable in most
cases. However, results may vary.

Note that these functions are never implicitly called for the driver. The driver
is always responsible for deciding when and if to call these.


pci_save_state
--------------

Usage:
	pci_save_state(dev, buffer);

Description:
	Save first 64 bytes of PCI config space. Buffer must be allocated by
	caller.


pci_restore_state
-----------------

Usage:
	pci_restore_state(dev, buffer);

Description:
	Restore previously saved config space. (First 64 bytes only);

	If buffer is NULL, then restore what information we know about the
	device from bootup: BARs and interrupt line.


pci_set_power_state
-------------------

Usage:
	pci_set_power_state(dev, state);

Description:
	Transition device to low power state using PCI PM Capabilities
	registers.

	Will fail under one of the following conditions:
	- If state is less than current state, but not D0 (illegal transition)
	- Device doesn't support PM Capabilities
	- Device does not support requested state


pci_enable_wake
---------------

Usage:
	pci_enable_wake(dev, state, enable);

Description:
	Enable device to generate PME# during low power state using PCI PM 
	Capabilities.

	Checks whether if device supports generating PME# from requested state
	and fail if it does not, unless enable == 0 (request is to disable wake
	events, which is implicit if it doesn't even support it in the first
	place).

	Note that the PMC Register in the device's PM Capabilties has a bitmask
	of the states it supports generating PME# from. D3hot is bit 3 and
	D3cold is bit 4. So, while a value of 4 as the state may not seem
	semantically correct, it is. 


4. PCI Device Drivers
~~~~~~~~~~~~~~~~~~~~~

These functions are intended for use by individual drivers, and are defined in 
struct pci_driver:

        int  (*save_state) (struct pci_dev *dev, u32 state);
        int  (*suspend) (struct pci_dev *dev, u32 state);
        int  (*resume) (struct pci_dev *dev);
        int  (*enable_wake) (struct pci_dev *dev, u32 state, int enable);


save_state
----------

Usage:

if (dev->driver && dev->driver->save_state)
	dev->driver->save_state(dev,state);

The driver should use this callback to save device state. It should take into
account the current state of the device and the requested state in order to
avoid any unnecessary operations.

For example, a video card that supports all 4 states (D0-D3), all controller
context is preserved when entering D1, but the screen is placed into a low power
state (blanked). 

The driver can also interpret this function as a notification that it may be
entering a sleep state in the near future. If it knows that the device cannot
enter the requested state, either because of lack of support for it, or because
the device is middle of some critical operation, then it should fail.

This function should not be used to set any state in the device or the driver
because the device may not actually enter the sleep state (e.g. another driver
later causes causes a global state transition to fail).

Note that in intermediate low power states, a device's I/O and memory spaces may
be disabled and may not be available in subsequent transitions to lower power
states.


suspend
-------

Usage:

if (dev->driver && dev->driver->suspend)
	dev->driver->suspend(dev,state);

A driver uses this function to actually transition the device into a low power
state. This may include disabling I/O, memory and bus-mastering, as well as
physically transitioning the device to a lower power state.

Bus mastering may be disabled by doing:

pci_disable_device(dev);

For devices that support the PCI PM Spec, this may be used to set the device's
power state:

pci_set_power_state(dev,state);

The driver is also responsible for disabling any other device-specific features
(e.g blanking screen, turning off on-card memory, etc).

The driver should be sure to track the current state of the device, as it may
obviate the need for some operations.

The driver should update the current_state field in its pci_dev structure in
this function.

resume
------

Usage:

if (dev->driver && dev->driver->suspend)
	dev->driver->resume(dev)

The resume callback may be called from any power state, and is always meant to
transition the device to the D0 state. 

The driver is responsible for reenabling any features of the device that had
been disabled during previous suspend calls and restoring all state that was
saved in previous save_state calls.

If the device is currently in D3, it must be completely reinitialized, as it
must be assumed that the device has lost all of its context (even that of its
PCI config space). For almost all current drivers, this means that the
initialization code that the driver does at boot must be separated out and
called again from the resume callback. Note that some values for the device may
not have to be probed for this time around if they are saved before entering the
low power state.

If the device supports the PCI PM Spec, it can use this to physically transition
the device to D0:

pci_set_power_state(dev,0);

Note that if the entire system is transitioning out of a global sleep state, all
devices will be placed in the D0 state, so this is not necessary. However, in
the event that the device is placed in the D3 state during normal operation,
this call is necessary. It is impossible to determine which of the two events is
taking place in the driver, so it is always a good idea to make that call.

The driver should take note of the state that it is resuming from in order to
ensure correct (and speedy) operation.

The driver should update the current_state field in its pci_dev structure in
this function.


enable_wake
-----------

Usage:

if (dev->driver && dev->driver->enable_wake)
	dev->driver->enable_wake(dev,state,enable);

This callback is generally only relevant for devices that support the PCI PM
spec and have the ability to generate a PME# (Power Management Event Signal)
to wake the system up. (However, it is possible that a device may support 
some non-standard way of generating a wake event on sleep.)

Bits 15:11 of the PMC (Power Mgmt Capabilities) Register in a device's
PM Capabilties describe what power states the device supports generating a 
wake event from:

+------------------+
|  Bit  |  State   |
+------------------+
|  15   |   D0     |
|  14   |   D1     |
|  13   |   D2     |
|  12   |   D3hot  |
|  11   |   D3cold |
+------------------+

A device can use this to enable wake events:

	 pci_enable_wake(dev,state,enable);

Note that to enable PME# from D3cold, a value of 4 should be passed to 
pci_enable_wake (since it uses an index into a bitmask). If a driver gets
a request to enable wake events from D3, two calls should be made to 
pci_enable_wake (one for both D3hot and D3cold).


5. Resources
~~~~~~~~~~~~

PCI Local Bus Specification 
PCI Bus Power Management Interface Specification

  http://pcisig.org

