This file contains brief information about the SCSI tape driver.
The driver is currently maintained by Kai Mäkisara (email
Kai.Makisara@kolumbus.fi)

Last modified: Sun Apr  6 22:44:55 2003 by makisara


BASICS

The driver is generic, i.e., it does not contain any code tailored
to any specific tape drive. The tape parameters can be specified with
one of the following three methods:

1. Each user can specify the tape parameters he/she wants to use
directly with ioctls. This is administratively a very simple and
flexible method and applicable to single-user workstations. However,
in a multiuser environment the next user finds the tape parameters in
state the previous user left them.

2. The system manager (root) can define default values for some tape
parameters, like block size and density using the MTSETDRVBUFFER ioctl.
These parameters can be programmed to come into effect either when a
new tape is loaded into the drive or if writing begins at the
beginning of the tape. The second method is applicable if the tape
drive performs auto-detection of the tape format well (like some
QIC-drives). The result is that any tape can be read, writing can be
continued using existing format, and the default format is used if
the tape is rewritten from the beginning (or a new tape is written
for the first time). The first method is applicable if the drive
does not perform auto-detection well enough and there is a single
"sensible" mode for the device. An example is a DAT drive that is
used only in variable block mode (I don't know if this is sensible
or not :-).

The user can override the parameters defined by the system
manager. The changes persist until the defaults again come into
effect.

3. Up to four modes can be defined and selected using the minor number
(bits 5 and 6). Mode 0 corresponds to the defaults discussed
above. Additional modes are dormant until they are defined by the
system manager (root). When specification of a new mode is started,
the configuration of mode 0 is used to provide a starting point for
definition of the new mode.

Using the modes allows the system manager to give the users choices
over some of the buffering parameters not directly accessible to the
users (buffered and asynchronous writes). The modes also allow choices
between formats in multi-tape operations (the explicitly overridden
parameters are reset when a new tape is loaded).

If more than one mode is used, all modes should contain definitions
for the same set of parameters.

Many Unices contain internal tables that associate different modes to
supported devices. The Linux SCSI tape driver does not contain such
tables (and will not do that in future). Instead of that, a utility
program can be made that fetches the inquiry data sent by the device,
scans its database, and sets up the modes using the ioctls. Another
alternative is to make a small script that uses mt to set the defaults
tailored to the system.

The driver supports fixed and variable block size (within buffer
limits). Both the auto-rewind (minor equals device number) and
non-rewind devices (minor is 128 + device number) are implemented.

In variable block mode, the byte count in write() determines the size
of the physical block on tape. When reading, the drive reads the next
tape block and returns to the user the data if the read() byte count
is at least the block size. Otherwise, error ENOMEM is returned.

In fixed block mode, the data transfer between the drive and the
driver is in multiples of the block size. The write() byte count must
be a multiple of the block size. This is not required when reading but
may be advisable for portability.

Support is provided for changing the tape partition and partitioning
of the tape with one or two partitions. By default support for
partitioned tape is disabled for each driver and it can be enabled
with the ioctl MTSETDRVBUFFER.

By default the driver writes one filemark when the device is closed after
writing and the last operation has been a write. Two filemarks can be
optionally written. In both cases end of data is signified by
returning zero bytes for two consecutive reads.

The compile options are defined in the file linux/drivers/scsi/st_options.h.


BSD AND SYS V SEMANTICS

The user can choose between these two behaviours of the tape driver by
defining the value of the symbol ST_SYSV. The semantics differ when a
file being read is closed. The BSD semantics leaves the tape where it
currently is whereas the SYS V semantics moves the tape past the next
filemark unless the filemark has just been crossed.

The default is BSD semantics.


BUFFERING

The driver uses tape buffers allocated either at system initialization
or at run-time when needed. One buffer is used for each open tape
device. The size of the buffers is selectable at compile and/or boot
time. The buffers are used to store the data being transferred to/from
the SCSI adapter. The following buffering options are selectable at
compile time and/or at run time (via ioctl):

Buffering of data across write calls in fixed block mode (define
ST_BUFFER_WRITES).

Asynchronous writing. Writing the buffer contents to the tape is
started and the write call returns immediately. The status is checked
at the next tape operation. Applies only to variable block mode.

Buffered writes and asynchronous writes may in some rare cases cause
problems in multivolume operations if there is not enough space on the
tape after the early-warning mark to flush the driver buffer.

Read ahead for fixed block mode (ST_READ_AHEAD). Filling the buffer is
attempted even if the user does not want to get all of the data at
this read command. Should be disabled for those drives that don't like
a filemark to truncate a read request or that don't like backspacing.

The buffer size is defined (in 1024 byte units) by ST_BUFFER_BLOCKS or
at boot time. If this size is not large enough, the driver tries to
temporarily enlarge the buffer. Buffer allocation uses chunks of
memory having sizes 2^n * (page size). Because of this the actual
buffer size may be larger than the buffer size specified with
ST_BUFFER_BLOCKS.

A small number of buffers are allocated at driver initialisation. The
maximum number of these buffers is defined by ST_MAX_BUFFERS. The
maximum can be changed with kernel or module startup options. One
buffer is allocated for each drive detected when the driver is
initialized up to the maximum.

The driver tries to allocate new buffers at run-time if
necessary. These buffers are freed after use. If the maximum number of
initial buffers is set to zero, all buffer allocation is done at
run-time. The advantage of run-time allocation is that memory is not
wasted for buffers not being used. The disadvantage is that there may
not be memory available at the time when a buffer is needed for the
first time (once a buffer is allocated, it is not released). This risk
should not be big if the tape drive is connected to a PCI adapter that
supports scatter/gather (the allocation is not limited to "DMA memory"
and the buffer can be composed of several fragments).

Scatter/gather buffers (buffers that consist of chunks non-contiguous
in the physical memory) are used if contiguous buffers can't be
allocated. To support all SCSI adapters (including those not
supporting scatter/gather), buffer allocation is using the following
three kinds of chunks:
1. The initial segment that is used for all SCSI adapters including
those not supporting scatter/gather. The size of this buffer will be
(PAGE_SIZE << ST_FIRST_ORDER) bytes if the system can give a chunk of
this size (and it is not larger than the buffer size specified by
ST_BUFFER_BLOCKS). If this size is not available, the driver halves
the size and tries again until the size of one page. The default
settings in st_options.h make the driver to try to allocate all of the
buffer as one chunk.
2. The scatter/gather segments to fill the specified buffer size are
allocated so that as many segments as possible are used but the number
of segments does not exceed ST_FIRST_SG.
3. The remaining segments between ST_MAX_SG (or the module parameter
max_sg_segs) and the number of segments used in phases 1 and 2
are used to extend the buffer at run-time if this is necessary. The
number of scatter/gather segments allowed for the SCSI adapter is not
exceeded if it is smaller than the maximum number of scatter/gather
segments specified. If the maximum number allowed for the SCSI adapter
is smaller than the number of segments used in phases 1 and 2,
extending the buffer will always fail.


MODULE PARAMETERS

The buffer size, write threshold, and the maximum number of allocated buffers
are configurable when the driver is loaded as a module. The keywords are:

buffer_kbs=xxx             the buffer size in kilobytes is set to xxx
max_buffers=xxx            the maximum number of tape buffer set to xxx
max_sg_segs=xxx		   the maximum number of scatter/gather
			   segments
blocking_open=xxx	   block in open() if drive not ready, O_NONBLOCK
			   not used, and blocking_open non-zero

Note that if the buffer size is changed but the write threshold is not
set, the write threshold is set to the new buffer size - 2 kB.


BOOT TIME CONFIGURATION

If the driver is compiled into the kernel, the same parameters can be
also set using, e.g., the LILO command line. The preferred syntax is
to use the same keywords as when loading the driver as module. If
several parameters are set, the keyword-value pairs are separated with
a comma (no spaces allowed). A colon can be used instead of the equal
mark. The definition is prepended by the string st=. Here is an
example:

	st=buffer_kbs:64,max_buffers:2

The following syntax used by the old kernel versions is also supported:

           st=aa[,bb[,cc[,dd]]]

where
  aa is the buffer size in 1024 byte units
  bb is the write threshold in 1024 byte units (not used any more)
  cc is the maximum number of tape buffers to allocate (the number of
        buffers is bounded also by the number of drives detected)
  dd is the maximum number of scatter/gather segments


IOCTLS

The tape is positioned and the drive parameters are set with ioctls
defined in mtio.h The tape control program 'mt' uses these ioctls. Try
to find an mt that supports all of the Linux SCSI tape ioctls and
opens the device for writing if the tape contents will be modified
(look for a package mt-st* from the Linux ftp sites; the GNU mt does
not open for writing for, e.g., erase).

The supported ioctls are:

The following use the structure mtop:

MTFSF   Space forward over count filemarks. Tape positioned after filemark.
MTFSFM  As above but tape positioned before filemark.
MTBSF	Space backward over count filemarks. Tape positioned before
        filemark.
MTBSFM  As above but ape positioned after filemark.
MTFSR   Space forward over count records.
MTBSR   Space backward over count records.
MTFSS   Space forward over count setmarks.
MTBSS   Space backward over count setmarks.
MTWEOF  Write count filemarks.
MTWSM   Write count setmarks.
MTREW   Rewind tape.
MTOFFL  Set device off line (often rewind plus eject).
MTNOP   Do nothing except flush the buffers.
MTRETEN Re-tension tape.
MTEOM   Space to end of recorded data.
MTERASE Erase tape.
MTSEEK	Seek to tape block count. Uses Tandberg-compatible seek (QFA)
        for SCSI-1 drives and SCSI-2 seek for SCSI-2 drives. The file and
	block numbers in the status are not valid after a seek.
MTSETBLK Set the drive block size. Setting to zero sets the drive into
        variable block mode (if applicable).
MTSETDENSITY Sets the drive density code to arg. See drive
        documentation for available codes.
MTLOCK and MTUNLOCK Explicitly lock/unlock the tape drive door.
MTLOAD and MTUNLOAD Explicitly load and unload the tape. If the
	command argument x is between MT_ST_HPLOADER_OFFSET + 1 and
	MT_ST_HPLOADER_OFFSET + 6, the number x is used sent to the
	drive with the command and it selects the tape slot to use of
	HP C1553A changer.
MTCOMPRESSION Sets compressing or uncompressing drive mode using the
	SCSI mode page 15. Note that some drives other methods for
	control of compression. Some drives (like the Exabytes) use
	density codes for compression control. Some drives use another
	mode page but this page has not been implemented in the
	driver. Some drives without compression capability will accept
	any compression mode without error.
MTSETPART Moves the tape to the partition given by the argument at the
	next tape operation. The block at which the tape is positioned
	is the block where the tape was previously positioned in the
	new active partition unless the next tape operation is
	MTSEEK. In this case the tape is moved directly to the block
	specified by MTSEEK. MTSETPART is inactive unless
	MT_ST_CAN_PARTITIONS set.
MTMKPART Formats the tape with one partition (argument zero) or two
	partitions (the argument gives in megabytes the size of
	partition 1 that is physically the first partition of the
	tape). The drive has to support partitions with size specified
	by the initiator. Inactive unless MT_ST_CAN_PARTITIONS set.
MTSETDRVBUFFER
	Is used for several purposes. The command is obtained from count
        with mask MT_SET_OPTIONS, the low order bits are used as argument.
	This command is only allowed for the superuser (root). The
	subcommands are:
	0
           The drive buffer option is set to the argument. Zero means
           no buffering.
        MT_ST_BOOLEANS
           Sets the buffering options. The bits are the new states
           (enabled/disabled) the following options (in the
	   parenthesis is specified whether the option is global or
	   can be specified differently for each mode):
	     MT_ST_BUFFER_WRITES write buffering (mode)
	     MT_ST_ASYNC_WRITES asynchronous writes (mode)
             MT_ST_READ_AHEAD  read ahead (mode)
             MT_ST_TWO_FM writing of two filemarks (global)
	     MT_ST_FAST_EOM using the SCSI spacing to EOD (global)
	     MT_ST_AUTO_LOCK automatic locking of the drive door (global)
             MT_ST_DEF_WRITES the defaults are meant only for writes (mode)
	     MT_ST_CAN_BSR backspacing over more than one records can
		be used for repositioning the tape (global)
	     MT_ST_NO_BLKLIMS the driver does not ask the block limits
		from the drive (block size can be changed only to
		variable) (global)
	     MT_ST_CAN_PARTITIONS enables support for partitioned
		tapes (global)
	     MT_ST_SCSI2LOGICAL the logical block number is used in
		the MTSEEK and MTIOCPOS for SCSI-2 drives instead of
		the device dependent address. It is recommended to set
		this flag unless there are tapes using the device
		dependent (from the old times) (global)
	     MT_ST_SYSV sets the SYSV sematics (mode)
	     MT_ST_NOWAIT enables immediate mode (i.e., don't wait for
	        the command to finish) for some commands (e.g., rewind)
	     MT_ST_DEBUGGING debugging (global; debugging must be
		compiled into the driver)
	MT_ST_SETBOOLEANS
	MT_ST_CLEARBOOLEANS
	   Sets or clears the option bits.
	MT_ST_DEF_BLKSIZE
	   Defines the default block size set automatically. Value
	   0xffffff means that the default is not used any more.
	MT_ST_DEF_DENSITY
	MT_ST_DEF_DRVBUFFER
	   Used to set or clear the density (8 bits), and drive buffer
	   state (3 bits). If the value is MT_ST_CLEAR_DEFAULT
	   (0xfffff) the default will not be used any more. Otherwise
	   the lowermost bits of the value contain the new value of
	   the parameter.
	MT_ST_DEF_COMPRESSION
	   The compression default will not be used if the value of
	   the lowermost byte is 0xff. Otherwise the lowermost bit
	   contains the new default. If the bits 8-15 are set to a
	   non-zero number, and this number is not 0xff, the number is
	   used as the compression algorithm. The value
	   MT_ST_CLEAR_DEFAULT can be used to clear the compression
	   default.
	MT_ST_SET_TIMEOUT
	   Set the normal timeout in seconds for this device. The
	   default is 900 seconds (15 minutes). The timeout should be
	   long enough for the retries done by the device while
	   reading/writing.
	MT_ST_SET_LONG_TIMEOUT
	   Set the long timeout that is used for operations that are
	   known to take a long time. The default is 14000 seconds
	   (3.9 hours). For erase this value is further multiplied by
	   eight.
	MT_ST_SET_CLN
	   Set the cleaning request interpretation parameters using
	   the lowest 24 bits of the argument. The driver can set the
	   generic status bit GMT_CLN if a cleaning request bit pattern
	   is found from the extended sense data. Many drives set one or
	   more bits in the extended sense data when the drive needs
	   cleaning. The bits are device-dependent. The driver is
	   given the number of the sense data byte (the lowest eight
	   bits of the argument; must be >= 18 (values 1 - 17
	   reserved) and <= the maximum requested sense data sixe), 
	   a mask to select the relevant bits (the bits 9-16), and the
	   bit pattern (bits 17-23). If the bit pattern is zero, one
	   or more bits under the mask indicate cleaning request. If
	   the pattern is non-zero, the pattern must match the masked
	   sense data byte.

	   (The cleaning bit is set if the additional sense code and
	   qualifier 00h 17h are seen regardless of the setting of
	   MT_ST_SET_CLN.)

The following ioctl uses the structure mtpos:
MTIOCPOS Reads the current position from the drive. Uses
        Tandberg-compatible QFA for SCSI-1 drives and the SCSI-2
        command for the SCSI-2 drives.

The following ioctl uses the structure mtget to return the status:
MTIOCGET Returns some status information.
        The file number and block number within file are returned. The
        block is -1 when it can't be determined (e.g., after MTBSF).
        The drive type is either MTISSCSI1 or MTISSCSI2.
        The number of recovered errors since the previous status call
        is stored in the lower word of the field mt_erreg.
        The current block size and the density code are stored in the field
        mt_dsreg (shifts for the subfields are MT_ST_BLKSIZE_SHIFT and
        MT_ST_DENSITY_SHIFT).
	The GMT_xxx status bits reflect the drive status. GMT_DR_OPEN
	is set if there is no tape in the drive. GMT_EOD means either
	end of recorded data or end of tape. GMT_EOT means end of tape.


MISCELLANEOUS COMPILE OPTIONS

The recovered write errors are considered fatal if ST_RECOVERED_WRITE_FATAL
is defined.

By default, open() does not block if the drive is not ready. The
behaviour can be changed by setting ST_BLOCKING_OPEN to one. The
behaviour can be changed also with the boot/module option
blocking_open. The blocking open times out after ST_BLOCK_SECONDS.

The maximum number of tape devices is determined by the define
ST_MAX_TAPES. If more tapes are detected at driver initialization, the
maximum is adjusted accordingly.

Immediate return from tape positioning SCSI commands can be enabled by
defining ST_NOWAIT. If this is defined, the user should take care that
the next tape operation is not started before the previous one has
finished. The drives and SCSI adapters should handle this condition
gracefully, but some drive/adapter combinations are known to hang the
SCSI bus in this case.

The MTEOM command is by default implemented as spacing over 32767
filemarks. With this method the file number in the status is
correct. The user can request using direct spacing to EOD by setting
ST_FAST_EOM 1 (or using the MT_ST_OPTIONS ioctl). In this case the file
number will be invalid.

When using read ahead or buffered writes the position within the file
may not be correct after the file is closed (correct position may
require backspacing over more than one record). The correct position
within file can be obtained if ST_IN_FILE_POS is defined at compile
time or the MT_ST_CAN_BSR bit is set for the drive with an ioctl.
(The driver always backs over a filemark crossed by read ahead if the
user does not request data that far.)


DEBUGGING HINTS

To enable debugging messages, edit st.c and #define DEBUG 1. As seen
above, debugging can be switched off with an ioctl if debugging is
compiled into the driver. The debugging output is not voluminuous.

If the tape seems to hang, I would be very interested to hear where
the driver is waiting. With the command 'ps -l' you can see the state
of the process using the tape. If the state is D, the process is
waiting for something. The field WCHAN tells where the driver is
waiting. If you have the current System.map in the correct place (in
/boot for the procps I use) or have updated /etc/psdatabase (for kmem
ps), ps writes the function name in the WCHAN field. If not, you have
to look up the function from System.map.

Note also that the timeouts are very long compared to most other
drivers. This means that the Linux driver may appear hung although the
real reason is that the tape firmware has got confused.
