<!DOCTYPE book PUBLIC "-//OASIS//DTD DocBook V3.1//EN"[]>

<book id="libataDevGuide">
 <bookinfo>
  <title>libATA Developer's Guide</title>
  
  <authorgroup>
   <author>
    <firstname>Jeff</firstname>
    <surname>Garzik</surname>
   </author>
  </authorgroup>

  <copyright>
   <year>2003</year>
   <holder>Jeff Garzik</holder>
  </copyright>

  <legalnotice>
   <para>
   The contents of this file are subject to the Open
   Software License version 1.1 that can be found at
   <ulink url="http://www.opensource.org/licenses/osl-1.1.txt">http://www.opensource.org/licenses/osl-1.1.txt</ulink> and is included herein
   by reference.
   </para>

   <para>
   Alternatively, the contents of this file may be used under the terms
   of the GNU General Public License version 2 (the "GPL") as distributed
   in the kernel source COPYING file, in which case the provisions of
   the GPL are applicable instead of the above.  If you wish to allow
   the use of your version of this file only under the terms of the
   GPL and not to allow others to use your version of this file under
   the OSL, indicate your decision by deleting the provisions above and
   replace them with the notice and other provisions required by the GPL.
   If you do not delete the provisions above, a recipient may use your
   version of this file under either the OSL or the GPL.
   </para>

  </legalnotice>
 </bookinfo>

<toc></toc>

  <chapter id="libataThanks">
     <title>Thanks</title>
  <para>
  The bulk of the ATA knowledge comes thanks to long conversations with
  Andre Hedrick (www.linux-ide.org).
  </para>
  <para>
  Thanks to Alan Cox for pointing out similarities 
  between SATA and SCSI, and in general for motivation to hack on
  libata.
  </para>
  <para>
  libata's device detection
  method, ata_pio_devchk, and in general all the early probing was
  based on extensive study of Hale Landis's probe/reset code in his
  ATADRVR driver (www.ata-atapi.com).
  </para>
  </chapter>

  <chapter id="libataDriverApi">
     <title>libata Driver API</title>
     <sect1>
        <title>struct ata_port_operations</title>

	<programlisting>
void (*port_disable) (struct ata_port *);
	</programlisting>

	<para>
	Called from ata_bus_probe() and ata_bus_reset() error paths,
	as well as when unregistering from the SCSI module (rmmod, hot
	unplug).
	</para>

	<programlisting>
void (*dev_config) (struct ata_port *, struct ata_device *);
	</programlisting>

	<para>
	Called after IDENTIFY [PACKET] DEVICE is issued to each device
	found.  Typically used to apply device-specific fixups prior to
	issue of SET FEATURES - XFER MODE, and prior to operation.
	</para>

	<programlisting>
void (*set_piomode) (struct ata_port *, struct ata_device *);
void (*set_dmamode) (struct ata_port *, struct ata_device *);
void (*post_set_mode) (struct ata_port *ap);
	</programlisting>

	<para>
	Hooks called prior to the issue of SET FEATURES - XFER MODE
	command.  dev->pio_mode is guaranteed to be valid when
	->set_piomode() is called, and dev->dma_mode is guaranteed to be
	valid when ->set_dmamode() is called.  ->post_set_mode() is
	called unconditionally, after the SET FEATURES - XFER MODE
	command completes successfully.
	</para>

	<para>
	->set_piomode() is always called (if present), but
	->set_dma_mode() is only called if DMA is possible.
	</para>

	<programlisting>
void (*tf_load) (struct ata_port *ap, struct ata_taskfile *tf);
void (*tf_read) (struct ata_port *ap, struct ata_taskfile *tf);
	</programlisting>

	<para>
	->tf_load() is called to load the given taskfile into hardware
	registers / DMA buffers.  ->tf_read() is called to read the
	hardware registers / DMA buffers, to obtain the current set of
	taskfile register values.
	</para>

	<programlisting>
void (*exec_command)(struct ata_port *ap, struct ata_taskfile *tf);
	</programlisting>

	<para>
	causes an ATA command, previously loaded with
	->tf_load(), to be initiated in hardware.
	</para>

	<programlisting>
u8   (*check_status)(struct ata_port *ap);
void (*dev_select)(struct ata_port *ap, unsigned int device);
	</programlisting>

	<para>
	Reads the Status ATA shadow register from hardware.  On some
	hardware, this has the side effect of clearing the interrupt
	condition.
	</para>

	<programlisting>
void (*dev_select)(struct ata_port *ap, unsigned int device);
	</programlisting>

	<para>
	Issues the low-level hardware command(s) that causes one of N
	hardware devices to be considered 'selected' (active and
	available for use) on the ATA bus.
	</para>

	<programlisting>
void (*phy_reset) (struct ata_port *ap);
	</programlisting>

	<para>
	The very first step in the probe phase.  Actions vary depending
	on the bus type, typically.  After waking up the device and probing
	for device presence (PATA and SATA), typically a soft reset
	(SRST) will be performed.  Drivers typically use the helper
	functions ata_bus_reset() or sata_phy_reset() for this hook.
	</para>

	<programlisting>
void (*bmdma_setup) (struct ata_queued_cmd *qc);
void (*bmdma_start) (struct ata_queued_cmd *qc);
	</programlisting>

	<para>
	When setting up an IDE BMDMA transaction, these hooks arm
	(->bmdma_setup) and fire (->bmdma_start) the hardware's DMA
	engine.
	</para>

	<programlisting>
void (*qc_prep) (struct ata_queued_cmd *qc);
int (*qc_issue) (struct ata_queued_cmd *qc);
	</programlisting>

	<para>
	Higher-level hooks, these two hooks can potentially supercede
	several of the above taskfile/DMA engine hooks.  ->qc_prep is
	called after the buffers have been DMA-mapped, and is typically
	used to populate the hardware's DMA scatter-gather table.
	Most drivers use the standard ata_qc_prep() helper function, but
	more advanced drivers roll their own.
	</para>
	<para>
	->qc_issue is used to make a command active, once the hardware
	and S/G tables have been prepared.  IDE BMDMA drivers use the
	helper function ata_qc_issue_prot() for taskfile protocol-based
	dispatch.  More advanced drivers roll their own ->qc_issue
	implementation, using this as the "issue new ATA command to
	hardware" hook.
	</para>

	<programlisting>
void (*eng_timeout) (struct ata_port *ap);
	</programlisting>

	<para>
	This is a high level error handling function, called from the
	error handling thread, when a command times out.
	</para>

	<programlisting>
irqreturn_t (*irq_handler)(int, void *, struct pt_regs *);
void (*irq_clear) (struct ata_port *);
	</programlisting>

	<para>
	->irq_handler is the interrupt handling routine registered with
	the system, by libata.  ->irq_clear is called during probe just
	before the interrupt handler is registered, to be sure hardware
	is quiet.
	</para>

	<programlisting>
u32 (*scr_read) (struct ata_port *ap, unsigned int sc_reg);
void (*scr_write) (struct ata_port *ap, unsigned int sc_reg,
                   u32 val);
	</programlisting>

	<para>
	Read and write standard SATA phy registers.  Currently only used
	if ->phy_reset hook called the sata_phy_reset() helper function.
	</para>

	<programlisting>
int (*port_start) (struct ata_port *ap);
void (*port_stop) (struct ata_port *ap);
void (*host_stop) (struct ata_host_set *host_set);
	</programlisting>

	<para>
	->port_start() is called just after the data structures for each
	port are initialized.  Typically this is used to alloc per-port
	DMA buffers / tables / rings, enable DMA engines, and similar
	tasks.  
	</para>
	<para>
	->host_stop() is called when the rmmod or hot unplug process
	begins.  The hook must stop all hardware interrupts, DMA
	engines, etc.
	</para>
	<para>
	->port_stop() is called after ->host_stop().  It's sole function
	is to release DMA/memory resources, now that they are no longer
	actively being used.
	</para>

     </sect1>
  </chapter>

  <chapter id="libataExt">
     <title>libata Library</title>
!Edrivers/scsi/libata-core.c
  </chapter>

  <chapter id="libataInt">
     <title>libata Core Internals</title>
!Idrivers/scsi/libata-core.c
  </chapter>

  <chapter id="libataScsiInt">
     <title>libata SCSI translation/emulation</title>
!Edrivers/scsi/libata-scsi.c
!Idrivers/scsi/libata-scsi.c
  </chapter>

  <chapter id="SILInt">
     <title>sata_sil Internals</title>
!Idrivers/scsi/sata_sil.c
  </chapter>

</book>
