
FORTH vocabulary
----------------
COLD            WARM            WIPE            RST_HERE        PWR_HERE        RST_STATE       PWR_STATE       
MOVE            LEAVE           +LOOP           LOOP            DO              REPEAT          WHILE           
AGAIN           UNTIL           BEGIN           THEN            ELSE            IF              >BODY           
DEFER           DOES>           CREATE          CONSTANT        VARIABLE        :               ;               
POSTPONE        RECURSE         IMMEDIATE       IS              [']             ]               [               
\               '               ABORT"          ABORT           QUIT            EVALUATE        COUNT           
LITERAL         ,               EXECUTE         >NUMBER         FIND            WORD            ."              
S"              CR              TYPE            SPACES          SPACE           NOECHO          ECHO            
EMIT            ACCEPT          KEY             C,              ALLOT           HERE            .               
D.              U.              SIGN            HOLD            #>              #S              #               
UM/MOD          <#              STATE           BASE            BL              J               I               
UNLOOP          U<              >               <               =               0<              0=              
DABS            1-              1+              1-              1+              -               +               
C!              C@              !               @               DEPTH           R@              R>              
>R              ROT             OVER            SWAP            NIP             DROP            ?DUP            
DUP             LIT             EXIT

COLD            Software reset

WARM            DEFERed word, by default executes ABORT" <WARM_message>"

WIPE            resets the program memory to its original state (Deep_RST adds same effect to COLD).

RST_HERE        defines the bound of the program memory protected against COLD or hardware reset.

PWR_HERE        defines the bound of the program memory protected against ON/OFF and also against any error occurring.

RST_STATE       removes all words defined after RST_HERE (COLD or <reset> have same effet)

PWR_STATE       removes all words defined after PWR_HERE (an occurring error has same effect)

MOVE            https://forth-standard.org/standard/core/MOVE
LEAVE           https://forth-standard.org/standard/core/LEAVE
+LOOP           https://forth-standard.org/standard/core/PlusLOOP
LOOP            https://forth-standard.org/standard/core/LOOP
DO              https://forth-standard.org/standard/core/DO        
REPEAT          https://forth-standard.org/standard/core/REPEAT
WHILE           https://forth-standard.org/standard/core/WHILE
AGAIN           https://forth-standard.org/standard/core/AGAIN
UNTIL           https://forth-standard.org/standard/core/UNTIL
BEGIN           https://forth-standard.org/standard/core/BEGIN
THEN            https://forth-standard.org/standard/core/THEN
ELSE            https://forth-standard.org/standard/core/ELSE
IF              https://forth-standard.org/standard/core/IF
;               https://forth-standard.org/standard/core/Semi
:               https://forth-standard.org/standard/core/Colon
DEFER           https://forth-standard.org/standard/core/DEFER
DOES>           https://forth-standard.org/standard/core/DOES
CREATE          https://forth-standard.org/standard/core/CREATE
CONSTANT        https://forth-standard.org/standard/core/CONSTANT
VARIABLE        https://forth-standard.org/standard/core/VARIABLE
POSTPONE        https://forth-standard.org/standard/core/POSTPONE
RECURSE         https://forth-standard.org/standard/core/RECURSE
IMMEDIATE       https://forth-standard.org/standard/core/IMMEDIATE
IS              https://forth-standard.org/standard/core/IS
[']             https://forth-standard.org/standard/core/BracketTick
]               https://forth-standard.org/standard/core/right-bracket
[               https://forth-standard.org/standard/core/Bracket
\               https://forth-standard.org/standard/block/bs
'               https://forth-standard.org/standard/core/Tick
ABORT"          https://forth-standard.org/standard/core/ABORTq
ABORT           https://forth-standard.org/standard/core/ABORT
QUIT            https://forth-standard.org/standard/core/QUIT
EVALUATE        https://forth-standard.org/standard/core/EVALUATE
COUNT           https://forth-standard.org/standard/core/COUNT
LITERAL         https://forth-standard.org/standard/core/LITERAL
,               https://forth-standard.org/standard/core/Comma
EXECUTE         https://forth-standard.org/standard/core/EXECUTE
>NUMBER         https://forth-standard.org/standard/core/toNUMBER
FIND            https://forth-standard.org/standard/core/FIND
WORD            https://forth-standard.org/standard/core/WORD
."              https://forth-standard.org/standard/core/Dotq
S"              https://forth-standard.org/standard/core/Sq
TYPE            https://forth-standard.org/standard/core/TYPE
SPACES          https://forth-standard.org/standard/core/SPACES
SPACE           https://forth-standard.org/standard/core/SPACE
CR              DEFERed word, https://forth-standard.org/standard/core/CR
NOECHO          stop display on output 
ECHO            start display on output
EMIT            DEFERed word, https://forth-standard.org/standard/core/EMIT
ACCEPT          DEFERed word, https://forth-standard.org/standard/core/ACCEPT
KEY             DEFERed word, https://forth-standard.org/standard/core/KEY
C,              https://forth-standard.org/standard/core/CComma
ALLOT           https://forth-standard.org/standard/core/ALLOT
HERE            https://forth-standard.org/standard/core/HERE
.               https://forth-standard.org/standard/core/d
D.              https://forth-standard.org/standard/double/Dd
U.              https://forth-standard.org/standard/core/Ud
SIGN            https://forth-standard.org/standard/core/SIGN
HOLD            https://forth-standard.org/standard/core/HOLD
#>              https://forth-standard.org/standard/core/num-end
#S              https://forth-standard.org/standard/core/numS
#               https://forth-standard.org/standard/core/num
UM/MOD          https://forth-standard.org/standard/core/UMDivMOD
<#              https://forth-standard.org/standard/core/num-start
BL              https://forth-standard.org/standard/core/BL
STATE           https://forth-standard.org/standard/core/STATE
BASE            https://forth-standard.org/standard/core/BASE
J               https://forth-standard.org/standard/core/J
I               https://forth-standard.org/standard/core/I
UNLOOP          https://forth-standard.org/standard/core/UNLOOP
U<              https://forth-standard.org/standard/core/Uless
>               https://forth-standard.org/standard/core/more
<               https://forth-standard.org/standard/core/less
=               https://forth-standard.org/standard/core/Equal
0<              https://forth-standard.org/standard/core/Zeroless
0=              https://forth-standard.org/standard/core/ZeroEqual
DABS            https://forth-standard.org/standard/double/DABS
ABS             https://forth-standard.org/standard/core/ABS
NEGATE          https://forth-standard.org/standard/core/NEGATE
1-              https://forth-standard.org/standard/core/OneMinus
1+              https://forth-standard.org/standard/core/OnePlus
-               https://forth-standard.org/standard/core/Minus
+               https://forth-standard.org/standard/core/Plus
C!              https://forth-standard.org/standard/core/CStore
C@              https://forth-standard.org/standard/core/CFetch
!               https://forth-standard.org/standard/core/Store
@               https://forth-standard.org/standard/core/Fetch
DEPTH           https://forth-standard.org/standard/core/DEPTH
R@              https://forth-standard.org/standard/core/RFetch
R>              https://forth-standard.org/standard/core/Rfrom
>R              https://forth-standard.org/standard/core/toR
ROT             https://forth-standard.org/standard/core/ROT
OVER            https://forth-standard.org/standard/core/OVER
SWAP            https://forth-standard.org/standard/core/SWAP
NIP             https://forth-standard.org/standard/core/NIP
DROP            https://forth-standard.org/standard/core/DROP
?DUP            https://forth-standard.org/standard/core/qDUP
DUP             https://forth-standard.org/standard/core/DUP
LIT             execution part of LITERAL            
EXIT            https://forth-standard.org/standard/core/EXIT


ASSEMBLER vocabulary
--------------------

?GOTO           GOTO            FW3             FW2             FW1             BW3             BW2             
BW1             ?JMP            JMP             REPEAT          WHILE           AGAIN           UNTIL           
ELSE            THEN            IF              0=              0<>             U>=             U<              
0<              0>=             S<              S>=             RRUM            RLAM            RRAM            
RRCM            POPM            PUSHM           CALL            PUSH.B          PUSH            SXT             
RRA.B           RRA             SWPB            RRC.B           RRC             AND.B           AND             
XOR.B           XOR             BIS.B           BIS             BIC.B           BIC             BIT.B           
BIT             DADD.B          DADD            CMP.B           CMP             SUB.B           SUB             
SUBC.B          SUBC            ADDC.B          ADDC            ADD.B           ADD             MOV.B           
MOV             RETI            LO2HI           COLON           ENDASM          ENDCODE         SLEEP

ASM             CODE            HI2LO           (added in forth vocabulary)

see: http://www.ece.utep.edu/courses/web3376/Notes_files/ee3376-isa.pdf
     readme.md for symbolic alias of registers, symbolic jumps (IF ELSE THEN...),..

?GOTO           used after a conditionnal (0=,0<>,U>=,U<,0<,S<,S>=) to branch to a label FWx or BWx
GOTO            used as unconditionnal branch to a label FWx or BWx

BW3             BACKWARD branch destination n°3
BW2                                         n°2
BW1                                         N°1

FW3             FORWARD branch destination  n°3
FW2                                         n°2
FW1                                         n°1

?JMP            used after a conditionnal (0=,0<>,U>=,U<,0<,S<,S>=) to jump to a predefined word
JMP             unconditionnal jump to a predefined word

REPEAT          assembler version of the FORTH word REPEAT
WHILE           idem
AGAIN           idem
UNTIL           idem
ELSE            idem
THEN            idem
IF              idem

0=              conditionnal     
0<>             conditionnal
U>=             conditionnal
U<              conditionnal
0<              conditionnal, to use only with ?JMP ?GOTO
0>=             conditionnal, to use only with IF UNTIL WHILE
S<              conditionnal
S>=             conditionnal

LO2HI           switches compilation between low level and high level modes without saving IP register.
COLON           pushes IP then performs LO2HI, used as: CODE <word> ... assembler instr ... COLON ... FORTH words ... ;
ENDASM          to end an ASM definition.
ENDCODE         to end a CODE definition.
SLEEP           DEFERed word which enables to create a background task, default SLEEP definition: MOV #GIE+LPM0,SR

next assembler words are set in FORTH vocabulary:

CODE <word>     creates a word written in assembler.
                this defined <word> must be ended with ENDCODE unless COLON or LO2HI use.

ASM <word>      creates a word written in assembler but not interpretable by FORTH (because ended by RET instr.).
                this defined <word> must be ended with ENDASM. 
                This word will be recognized only in assembler mode. 

HI2LO           used to switch compilation from high level (FORTH) to low level (assembler).


ASSEMBLER WORDS set:

ADD     http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=135
ADDC    http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=136
AND     http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=137
BIC     http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=138
BIS     http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=139
BIT     http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=140
CALL    http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=142
CMP     http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=147
DADD    http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=149
MOV     http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=165
PUSH    http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=168
RETI    http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=170
RRA     http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=173
RRC     http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=174
SUB     http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=179
SUBC    http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=180
SWPB    http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=181
SXT     http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=182
XOR     http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=184

RRUM    http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=218
RLAM    http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=208
RRAM    http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=211
RRCM    http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=214
POPM    http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=204
PUSHM   http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=205

ASSEMBLER_EXTENDED WORDS set:

ADDX    http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=187
ADDCX   http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=188
ANDX    http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=189
BICX    http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=190
BISX    http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=191
BITX    http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=192
CMPX    http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=194
DADDX   http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=196
MOVX    http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=202
PUSHX   http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=207
RRAX    http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=212
RRCX    http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=216
RRUX    http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=219
SUBX    http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=221
SUBCX   http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=222
SWPBX   http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=223
SXTX    http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=225
XORX    http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=227

ADDA    http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=229
CALLA   http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=232
CMPA    http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=235
MOVA    http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=238
SUBA    http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=241

RPT     http://www.ti.com/lit/ug/slau272d/slau272d.pdf#page=219

CONDCOMP ADD-ON
---------------
MARKER          [DEFINED]       [UNDEFINED]     [IF]            [ELSE]          [THEN]          COMPARE         

[DEFINED]       https://forth-standard.org/standard/tools/BracketDEFINED
[UNDEFINED]     https://forth-standard.org/standard/tools/BracketUNDEFINED
[IF]            https://forth-standard.org/standard/tools/BracketIF
[ELSE]          https://forth-standard.org/standard/tools/BracketELSE
[THEN]          https://forth-standard.org/standard/tools/BracketTHEN
COMPARE         https://forth-standard.org/standard/string/COMPARE
MARKER          https://forth-standard.org/standard/core/MARKER


VOCABULARY ADD-ON
-----------------
DEFINITIONS     ONLY            PREVIOUS        ALSO            ASSEMBLER       FORTH           VOCABULARY

DEFINITIONS     https://forth-standard.org/standard/search/DEFINITIONS
ONLY            https://forth-standard.org/standard/search/ONLY
PREVIOUS        https://forth-standard.org/standard/search/PREVIOUS
ALSO            https://forth-standard.org/standard/search/ALSO
ASSEMBLER       assembler VOCABULARY
FORTH           FORTH VOCABULARY
VOCABULARY <word>     creates a new VOCABULARY named word


NONAME ADD-ON
---------------------
:NONAME         CODENNM

:NONAME         https://forth-standard.org/standard/core/ColonNONAME 
CODENNM         assembly counterpart of :NONAME


SD_CARD_LOADER ADD-ON
---------------------
LOAD"           CIB

LOAD"           LOAD" SD_TEST.4TH" loads source file SD_TEST.4TH from SD_Card and compile it.
CIB             Currrent Input Buffer, TIB by default.

ACCEPT becomes a DEFERed word


SD_CARD_READ_WRITE ADD-ON
-------------------------
TERM2SD"        SD_EMIT         WRITE           READ            CLOSE           DEL"            WRITE"          
READ"

TERM2SD"        TERM2SD" SD_TEST.4TH" copy input file to SD_CARD (use CopySourceFileToTarget_SD_Card.bat to do)
SD_EMIT         sends output stream at the end of last opened as write file.
WRITE           write sequentially BUFFER content to a sector
READ            read sequentially a sector to BUFFER
CLOSE           close last opened file.
DEL"            DEL" SD_TEST.4TH" remove this file from SD_CARD.
WRITE"          WRITE" TRUC" open or create TRUC file ready to write to the end of this file
READ"           READ" TRUC" open TRUC and load its first sector in BUFFER



BOOTLOADER
----------
BOOT

QUIT becomes a DEFERed word


; when ADD-ONs are compiled into the kernel, their respective MARKER word identified with braces {} does nothing.
; when ADD-ONs are downloaded, their respective MARKER word identified with braces {} removes all ADD-ONs words.


ANS_COMPLEMENT ADD-ON
---------------------
PAD             >IN             SOURCE          .(              (               DECIMAL         HEX             
FILL            [CHAR]          CHAR            +!              MIN             MAX             2/              
2*              RSHIFT          LSHIFT          XOR             OR              AND             INVERT          
2OVER           2SWAP           2DROP           2DUP            2VALUE          2!              2@              
S>D             CELL+           CELLS           CHAR+           CHARS           ALIGN           ALIGNED         
*/              */MOD           MOD             /               /MOD            *               FM/MOD          
SM/REM          M*              UM*             TO              VALUE           {ANS_COMP}

PAD             https://forth-standard.org/standard/core/PAD            
>IN             https://forth-standard.org/standard/core/toIN
>BODY           https://forth-standard.org/standard/core/toBODY
SOURCE          https://forth-standard.org/standard/core/SOURCE
.(              https://forth-standard.org/standard/core/Dotp
(               https://forth-standard.org/standard/core/p
DECIMAL         https://forth-standard.org/standard/core/DECIMAL
HEX             https://forth-standard.org/standard/core/HEX
FILL            https://forth-standard.org/standard/core/FILL
[CHAR]          https://forth-standard.org/standard/core/BracketCHAR
CHAR            https://forth-standard.org/standard/core/CHAR
+!              https://forth-standard.org/standard/core/PlusStore
2/              https://forth-standard.org/standard/core/TwoDiv
2*              https://forth-standard.org/standard/core/TwoTimes
MIN             https://forth-standard.org/standard/core/MIN
MAX             https://forth-standard.org/standard/core/MAX
RSHIFT          https://forth-standard.org/standard/core/RSHIFT
LSHIFT          https://forth-standard.org/standard/core/LSHIFT
INVERT          https://forth-standard.org/standard/core/INVERT
XOR             https://forth-standard.org/standard/core/XOR
OR              https://forth-standard.org/standard/core/OR
AND             https://forth-standard.org/standard/core/AND
2OVER           https://forth-standard.org/standard/core/TwoOVER
2SWAP           https://forth-standard.org/standard/core/TwoSWAP
2DROP           https://forth-standard.org/standard/core/TwoDROP
2DUP            https://forth-standard.org/standard/core/TwoDUP
2VALUE          https://forth-standard.org/standard/double/TwoVALUE
2!              https://forth-standard.org/standard/core/TwoStore
2@              https://forth-standard.org/standard/core/TwoFetch
S>D             https://forth-standard.org/standard/core/StoD
CELL+           https://forth-standard.org/standard/core/CELLPlus
CELLS           https://forth-standard.org/standard/core/CELLS
CHAR+           https://forth-standard.org/standard/core/CHARPlus
CHARS           https://forth-standard.org/standard/core/CHARS
ALIGN           https://forth-standard.org/standard/core/ALIGN
ALIGNED         https://forth-standard.org/standard/core/ALIGNED
*/              https://forth-standard.org/standard/core/TimesDiv
*/MOD           https://forth-standard.org/standard/core/TimesDivMOD
MOD             https://forth-standard.org/standard/core/MOD
/               https://forth-standard.org/standard/core/Div
/MOD            https://forth-standard.org/standard/core/DivMOD
*               https://forth-standard.org/standard/core/Times
FM/MOD          https://forth-standard.org/standard/core/FMDivMOD
SM/REM          https://forth-standard.org/standard/core/SMDivREM
M*              https://forth-standard.org/standard/core/MTimes
UM*             https://forth-standard.org/standard/core/UMTimes
TO              https://forth-standard.org/standard/core/TO
VALUE           https://forth-standard.org/standard/core/VALUE
{ANS_COMP}


FIXPOINT ADD-ON
---------------

2CONSTANT       S>F             F.              F*              F#S             
F/              F-              F+              HOLDS           {FIXPOINT}

2CONSTANT       https://forth-standard.org/standard/double/TwoCONSTANT
S>F             u/n -- Qlo Qhi       convert u/n in a s15.16 value
F.              display a s15.16 value
F*              s15.16 multiplication  
F#S             Qlo Qhi u -- Qhi 0    
                convert fractionnal part of a s15.16 value displaying u digits
F/              s15.16 division        
F-              s15.16 soustraction
F+              s15.16 addition
HOLDS           https://forth-standard.org/standard/core/HOLDS
{FIXPOINT}      do nothing if compiled in core, else remove all FIXPOINT add-on.

UTILITY ADD-ON
--------------

DUMP            U.R             WORDS           ?               .RS             .S              {TOOLS}

DUMP            https://forth-standard.org/standard/tools/DUMP  
U.R   u z --    display unsigned number u with size z
WORDS           https://forth-standard.org/standard/tools/WORDS 
?               https://forth-standard.org/standard/tools/q
.RS             displays return stack content
.S              https://forth-standard.org/standard/tools/DotS
{TOOLS}         do nothing if compiled in core.


SD_TOOLS ADD-ON
---------------

DIR             FAT             CLUSTER         SECTOR          {SD_TOOLS}

DIR             dump first sector of current directory
FAT             dump first sector of FAT1
CLUSTER         .123 CLUSTER displays first sector of cluster 123
SECTOR          .123456789 SECTOR displays sector 123456789
{SD_TOOLS}      if you type {SD_TOOLS}  all subsequent loaded words are removed


